### Controlling the robot

To control the CM-530 controller, I first needed to probe the RX line directly from the receiver on the robot’s head, and determine the actions needed to make it move up, down, left, and right. After figuring out that the baud rate of the receiver was 1900 baud, I recorded all of the values being transmitted via Logic Analyzer, and wrote up a quick sketch to test this.